# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of < Supply of a Garbage Bins > p 1 /…**

**Publication reference:** < TS/2020/421-733\_VM/Sup-04>

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | **plastic Container FOR PET Bottles** - Compliance to the EN840 standards  - Volume: 770 L  - Overall Length: 1300 mm (+/-10 %)  - Overall Height: 1300 mm (+/-10 %)  - Weight: 40 kg (+/-10 %)  - Quantity of wheels: 4 rubber (2 wheels with brake)  - Polyethylene container with minimum a one rubber valve.  - Circular opening for bottles diameter 200 mm (+/-10 %).  - Wheel diameter: 200 (+/-10 %)  - Material: virgin HDPE  - Colour: blue, yellow, green (the entire lot must be of one color and that color must not be repeated with a lot of bins of another size)  - Quantity: 630  The container body along the perimeter is reinforced with stiffeners. At the bottom there is a drain hole with a stopper and protection against falling out.  Container shall match the mechanized garbage truck with a back load. At the top the Waste Container has a lid. |  |  |  |
| **2** | **plastic Container for solid household waste** -Compliance to the EN840 standards  -Volume: 1100L  - Overall Length: 1300 mm (+/-10 %)  - Overall Height: 1300 mm (+/-10 %)  - Weight: 50 kg (+/-20 %)  - Quantity of wheels: 4 rubber (2 wheels with brake)  - Material: virgin HDPE  - Colour: blue, yellow, green (the entire lot must be of one color and that color must not be repeated with a lot of bins of another size)  - Round hole: radius 350  - Wheel diameter: 200 (+/-10 %)  - Quantity: 630  The container body along the perimeter is reinforced with stiffeners. At the bottom there is a drain hole with a stopper and protection against falling out.  Waste Container shall match the mechanized garbage truck with a back load. At the top the Waste Container has a lid. |  |  |  |